LC-SC Optical Fibre Cable OS2

**Overview**

Single mode fiber optic cable is suitable for enterprise network, Telecom rooms, server farms, cloud storage networks and any place where fiber jumper cables are needed. This cable is ideal for connecting 1G/10G/40G/100G Ethernet connections. It can transport data for up to 10km at 1310nm, or up to 40km at 1550nm. The single mode patch cords are manufactured using LSZH cables which conform to IEC, EIA TIA or Telcordia standards.



**Features**

* Designed for Data Centers, Industry and Computer Centers
* LSZH (Low Smoke Zero Halogen) and flame retardant
* RoHS compliant

**Technical Specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | *FIB2210XX* | **Specs** | *Supports speeds up to 1G/10G/40G/100G* |
| **Length** | *0,5m,1m,2m,3m,5m,7m,10m,15m,20m,25m* |  |  |
| **Material** | *LSZH Cable* |  |  |
| **Shielding** | *Single shielded* | **Warranty** | *30 Years* |
| **Common applications** | *For Data Centers, industry and computer centers.* | **Version** | *SC-SC Optical fibre Singlemode duplex OS2 cable.* |
|  |  |  |  |
|  |  | **Testing** | *Tested before shipment* |
|  |  |  |  |
| **Colors** | *Yellow* | **Packing** | *Clear plastic bag* |
|  |  | **Certifications** | *LSZH, RoHS* |
|  |  | **Installation and use** | *Plug and Play* |
|  |  |  | *Indoor* |

****