SC-SC Optical Fibre Cable OM5

**Overview**

Due to the demand of the continuously increasing bandwidth, the fiber patch cables also has updated quality. The latest version is Multimode OM5, also known as WBMMF (WideBrand MultiMode Fiber). This is made to meet the growing bandwidth requirements.

**Features**

* Designed for Data Centers, Industry and Computer Centers
* LSZH (Low Smoke Zero Halogen) and flame retardant
* RoHS compliant

**Technical Specification**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | *FIB5710XX* | **Specs** | *50/125µm OM5 multimode* |
| **Length** | *0,5m,1m,2m,3m,5m,7m,10m,15m,20m,25m* |  |  |
| **Material** | *LSZH Cable* |  |  |
| **Shielding** | *Single shielded* | **Warranty** | *30 Years* |
| **Common applications** | *For Data Centers, industry and computer centers.* | **Version** | *SC-SC Optical fibre Multimode duplex OM5 cable.* |
|  |  |  |  |
|  |  | **Testing** | *Tested before shipment* |
|  |  |  |  |
| **Colors** | *Green* | **Packing** | *Clear plastic bag* |
|  |  | **Certifications** | *LSZH, RoHS* |
|  |  | **Installation and use** | *Plug and Play* |
|  |  |  | *Indoor* |

****